Shivkumar Kalyanaraman

Rensselaer Polytechni c Instit ute

Informal Quiz 6

T F o o Video is different from data only because it requires larger bandwidth o o One reason TCP is not suitable for video is because it can´t handle multicast o o RTP provides useful transport functions for multimedia applications , but the internet service enhancement is provided by

RSVP, integrated services and differentiated services o o A delay guarantee can be provided by combining a leaky bucket at the edge, with weighted fair queueing at the routers o o RSVP is a reservation-based routing protocol o o Differentiated s ervices would provide better-than-bes t-effort service (where $$ define QoS ) in a s calable manner.

Shivkumar Kalyanaraman

Rensselaer Polytechni c Instit ute

Informal Quiz 6 ( contd )

T F o o Aggegatable global unicast address es in IPv6 allow better routing because aggregation is based on topology defined by providers and not geographic or political boundaries o o Link local addresses, multicast and neighbor discovery are key components in IPv6 which allow plug-and-play.

o o Flow class ification (bas ed on IP addresses and port numbers) cannot be done when the authentication header is used, but can be done when the payload is encapsulated (ESP is used).

o o The scope of the multicast is not a part of the IPv6 address.

Shivkumar Kalyanaraman

Rensselaer Polytechni c Instit ute

Informal Quiz 6: solutions

T F o

Ö Video is different from data only because it requires larger bandwidth

Ö o One reason TCP is not suitable for video is becaus e it cannot handle multicast

Ö o RTP provides useful transport functions for multimedia applications , but the internet service enhancement is provided by

RSVP, integrated services and differentiated services

Ö o A delay guarantee can be provided by combining a leaky bucket at the edge, with weighted fair queueing at the routers o

Ö RSVP is a reservation-based routing protocol

Ö o Differentiated services would provide better-than-best-effort service (where $$ define QoS ) in a s calable manner.

Shivkumar Kalyanaraman

Rensselaer Polytechni c Instit ute

Informal Quiz 6 solns ( contd )

T F

Ö o Aggegatable global unicast addresses in IPv6 allow better routing because aggregation is based on topology defined by providers and not geographic or political boundaries

Ö o Link local addres ses, multicast and neighbor discovery are key components in IPv6 which allow plug-and-play.

o

Ö Flow classification (based on IP addres ses and port numbers) cannot be done when the authentication header is used, but can be done when the payload is encaps ulated (ESP is used).

o

Ö The scope of the multicast is not a part of the IPv6 addres s.