Shivkumar Kalyanaraman

Rensselaer Polytechnic Institut e

1

Infor mal Quiz 1

True or False?

T F

The structure of MAC addresses facilitates

scalability in implementations.

The interface between layers often outlives the

technology used in each layer.

If a node is multi-homed, it must be configured as a

router

Heterogeneity and scale is the reason why routers

are required for internetworking.

A layer-2 switch connects two broadcast domains.

ARP and RARP run over IP

The protocol field in the PPP header is used for

demultiplexing

Shivkumar Kalyanaraman 2

The CRC field in Ethernet is found in the trailer

because there was no space in the header .

Meta -data about voice samples in telephony is in a

large part inferred from timing.

Statistical multiplexing is most useful when the

peak rate is close to the average rate

Shivkumar Kalyanaraman 3

Infor mal Quiz 1:Solutions

True or False?

T F

The structure of MAC addresses facilitates

scalability in implementations.

The interface between layers often outlives the

technology used in each layer.

If a node is multi-homed, it must be configured as a

router

Heterogeneity and scale is the reason why routers

are required for internetworking.

A layer-2 switch connects two broadcast domains.

ARP and RARP run over IP

The protocol field in the PPP header is used for

demultiplexing

Shivkumar Kalyanaraman 4

The CRC field in Ethernet is found in the trailer

because there was no space in the header .

Meta -data about voice samples in telephony is in a

large part inferred from timing.

Statistical multiplexing is most useful when the

peak rate is close to the average rate

Shivkumar Kalyanaraman 5

Infor mal Quiz 1: Solutions

True or False?

T F

A router is necessary to split a large Ethernet into multiple pieces for

performance

FTP and telnet are client-server protocols

Both IP and ATM have network layer functionality. So, when IP runs

over ATM, ATM´s full functionality is suppressed.

If a node is multi-homed, it must be configured as a router

In connection-oriented communication, you need to fix the path taken

from source to destination

The unique IP address of any network interface is assigned by InterNIC

ARP and RARP run over IP

The protocol field in the PPP header is used for demultiplexing

The CRC field in Ethernet is found in the trailer because there was no

space in the header .

Bridges demarcate the broadcast domain in an Ethernet LAN.

Marks = Correct Answers _____ - Incorrect Answers _____ = ______