Shivkumar Kalyanaraman

Rensselaer

Informal Quiz 3

True or False?

T F o o The Nagle algorithm in TCP is intended to allow the ack and echo data to be combined.

o o TCP is called ^self-clocking~ because the source sends a new packet into the network only upon receiving an ack .

o o TCP by default uses a go-back-N retransmission policy o o A reason why fast-retransmit results in low throughput due to bursty drop is because it performs multiplicative decrease for each of the packets lost.

o o TCP can control throughput & delay of a connection, and backs off during loss.

o o The RFC 793 RTT estimator could only tolerate variances of upto 30% o o Anything slower than a multiplicative decrease and anything faster than a linear increase of congestion window can lead to instability.

o o The slow-start exponential increase allows faster-than-linear increase and can work in general without congestion avoidance o o The persist timer is used by an ftp server to detect and close idle TCP connections o o Karn´s algorithm would be triggered often on a wireless or radio link.

o o Delayed- acks are good for interactive traffic, but bad for bulk traffic.

Marks = Correct Answers _____ - Incorrect Answers _____ = ______

Shivkumar Kalyanaraman

Rensselaer

Informal Quiz 3

True or False?

T F o Ö The Nagle algorithm in TCP allows the ack and echo data to be combined.

Ö o TCP is called ^self-clocking~ because the source sends a new packet into the network only upon receiving an ack .

Ö o TCP by default uses a go-back-N retransmission policy

Ö o A reason why fast-retransmit results in low throughput due to bursty drop is because it performs multiplicative decrease for each of the packets lost.

o Ö TCP can control throughput & delay of a connection, and backs off during loss.

Ö o The RFC 793 RTT estimator could only tolerate variances of upto 30%

Ö o Anything slower than a multiplicative decrease and anything faster than a linear increase of congestion window can lead to instability.

o Ö The slow-start exponential increase allows faster-than-linear increase and can work in general without congestion avoidance o

Ö The persist timer is used by an ftp server to detect and close idle TCP connections

Ö o Karn´s algorithm would be triggered often on a wireless or radio link.

Ö o Delayed- acks are good for interactive traffic, but bad for bulk traffic.

Marks = Correct Answers _____ - Incorrect Answers _____ = ______